**山东华盛中天工程机械有限责任公司**

**ND-40II Petrol Breaker**

|  |  |
| --- | --- |
| 产品代码 Product code | **ND-40II** |
| 发动机类型Engine Type | 单缸风冷二冲程Two-stroke, single cylinder, forced air-cooling |
| 功率Power (kw/r/min) | 2.0/6500 |
| 冲击频率Impact Number （Hz） | 12-25 |
| 冲击能Impact energy (J) | 45 |
|  |  |
| 工作转速Working rotating Speed (r.min) | 6000 |
| 包装尺寸Packing size (mm) | 950\*450\*450 |
| 净重Net Weight (kg) | 27.5 |
| 毛重Gross Weight (kg) | 33 |

**Product characteristics:**

1. The integrated two-stroke gasoline engine is used as the power. The structure is compact and the power is strong. It is widely used in road maintenance and tamping operations of railway track beds.

2. Adopt high-quality alloy leaf spring for shock absorption, with high strength, high wear resistance, sufficient emphasis and toughness, comfortable operation and low vibration.

3. Various operations such as tamping, crushing, shoveling, tamping, etc. can be carried out by replacing different accessories and tools, which can meet the requirements of railway maintenance, highway maintenance and civil engineering.