**山东华盛中天工程机械有限责任公司**

**HS950 Mini Road Roller**

|  |  |
| --- | --- |
| 规格型号Model | **HS950** |
| 配套动力Mating Power | 186F diesel |
| 发动机类型Engine Type | Single cylineder、air-cooled、4 Stroke 单缸、风冷、四冲程 |
| 功率Power | 6.3Kw/3600r/min |
| 油箱Fuel Tank | 15L |
| 燃油消耗Fuel Consumption | 1L/hour |
| 行走速度Walk Speed | 0-3km/hour |
| 理论爬坡能力Theoretical Grade Ability | 30% |
| 润滑油量 Oil Tank | 1.65L |
| 水箱Water Tank | 67L |
| 静线载荷Static Linear Load | 57/77N/cm |
| 名义振幅Nominal Amplitude | 0.5mm |
| 激振力Centrifugal Force | 20KN |
| 振动频率Vibration Frequency | 70Hz |
| 钢轮宽度Width of Steel Wheel | 700mm |
| 钢轮直径Diameter of Steel Wheel | 500mm |
| 驱动Drive | Hydraulic System |
| 振动Vibration | USA Danfoss hydraulic syetem,electromagnetic Cluch 美国萨奥液压泵 电磁离合振动 |
| 整机尺寸L\*W\*H (mm) | 1840\*840\*1820 |
| 净重 Net Weight | 950kg |
| 毛重Gross Weight | 1100kg |
| 包装箱尺寸（mm） | 2100\*970\*1620 |

**Product characteristics:**

Product characteristics:

1、This machine uses well-known brand gasoline engine or diesel engine as the power source, with strong power, reliable and durable.

2、Steel wheels made of manganese plate have a longer service life than steel wheels made of ordinary steel.

3、USA Danfoss hydraulic syetem and Taiwan electromagnetic clutch,the working performance is more stable,more convenient to use and reliable products.

4、NSK bearing and mitsuboshi V-belt.

5、comfortable driving seat

6、Plastic treated,anti-rust,anti-corrosion and beautiful.