Specifications for Disabled Tricycle XF110ZH-6C
Whole tricycle specification		
1	Engine type	Four stroke engines with single cylinder and air-cooled	
	Displacement(ml)	107	
2	Max power( Kw(r/min))	5.2 / 8500	
3	Dimension(mm)	2100*950*1100	
4	Wheel base(mm)	1580	
5	Complete vehicle weight (kg)	180	
6	Max. loading capacity(kg)	400	
7	Tyre	Front 3.75-12     Rear 4.00-12	
8	Starter	Electric / Kick	
9	Model of brake	Disc / Disc	
10	Max speed(km/h)	70	
11	Transmission	By shaft	
12	G.V.W(kg)	580	
13	Fuel consumption km per liter	2.8L/100KM