**Landing Gear**

Our landing gear, also called as trailer landing leg, is quite durable and easy to use both in freezing Siberia or the scorching Mid-East. The creative design of this trailer accessory can help you save time, fuel, working load, and even the potential safety risk can be reduced.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 型号  Model | 静载荷  Static  Load  (t/pair) | 承载能力  Capacity  (t/pair) | 侧向负载  Lateral  Force  Resistant  (t/pair) | 提升行程D  Maximum  Lift D  (mm) | 安装高度A  Closed  Height A  (mm) | 高速档  High Gear  Per Turn of  Handle  (mm/r) | 低速档  Low Gear  Per Turn of  Handle  (mm/r) | 重量  Weight  (kgs) |
| FSL60－25A | 60 | 25 | 12 | 480 | 840 | 6 | 0.7 | 94 |
| FSL60－25B | 60 | 25 | 12 | 430 | 791 | 6 | 0.7 | 90 |
| FSL80－28A | 80 | 28 | 14 | 480 | 840 | 6 | 0.67 | 108 |
| FSL80－28B | 80 | 28 | 14 | 430 | 789 | 6 | 0.67 | 104 |
| FSL80－28C | 80 | 28 | 14 | 355 | 713 | 6 | 0.67 | 98 |
| FSL80－28D | 80 | 28 | 13 | 480 | 840 | 6 | 0.7 | 94 |
| FSL80－28E | 80 | 28 | 13 | 430 | 790 | 6 | 0.7 | 91 |