**Landing Gear**

Our landing gear, also called as trailer landing leg, is quite durable and easy to use both in freezing Siberia or the scorching Mid-East. The creative design of this trailer accessory can help you save time, fuel, working load, and even the potential safety risk can be reduced.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 型号Model | 静载荷StaticLoad(t/pair)   | 承载能力Capacity(t/pair) | 侧向负载LateralForceResistant(t/pair) | 提升行程DMaximumLift D(mm) | 安装高度AClosedHeight A(mm) | 高速档High GearPer Turn ofHandle(mm/r) | 低速档Low GearPer Turn ofHandle(mm/r) | 重量Weight(kgs) |
| FSL60－25A | 60 | 25 | 12 | 480 | 840 | 6 | 0.7 | 94 |
| FSL60－25B | 60 | 25 | 12 | 430 | 791 | 6 | 0.7 | 90 |
| FSL80－28A | 80 | 28 | 14 | 480 | 840 | 6 | 0.67 | 108 |
| FSL80－28B | 80 | 28 | 14 | 430 | 789 | 6 | 0.67 | 104 |
| FSL80－28C | 80 | 28 | 14 | 355 | 713 | 6 | 0.67 | 98 |
| FSL80－28D | 80 | 28 | 13 | 480 | 840 | 6 | 0.7 | 94 |
| FSL80－28E | 80 | 28 | 13 | 430 | 790 | 6 | 0.7 | 91 |