**山东华盛中天工程机械有限责任公司**

**HZR106A Plate Compactor**

|  |  |
| --- | --- |
| 产品代码Product Code | **HZR106A** |
| 发动机型号Engine Model | 华盛EX17/168FA |
| 发动机类型Engine Type | Four-stroke, single cylinder, forced air-cooling |
| 排量Displacement (cc) | 163 |
| 冲击频率Impact Number/min | 90 |
| 冲击能 Impact Engerny (Kn) | 22 |
| 压实深度Press Depth (cm) | 30 (1.5 ton) |
| 行走速度Walk Speed(m/min) | 23 |
| 离合转速Clutch Revolution (r/min) | 2100 |
| 工作转速Work Revolution (r.min) | 3600 |
| 夯板尺寸 Base Dimension (mm) | 500\*490 |
| 包装尺寸Packing size (mm) | 860\*560\*730 |
| 净重Net Weight (kg) | 106 |
| 毛重Gross Weight (kg) | 116 |
| 包装方式Packing | Plywood (fumigation free) |

**Product characteristics:**

1. Ductile iron base plate provides better durability.

2、The vibration mechanism and the power part are connected by a high-elastic natural rubber shock absorption column, which is durable and comfortable to operate.

3、The tamper plate is made of ductile iron with high mechanical properties, strong impact resistance and good wear resistance.

4、 Centrally located lifting bar allows easy transportation.

5、Sealed belt cover to prevent sand and soil in.

6、Folding handles and wheels are added for easy transfer.