**山东华盛中天工程机械有限责任公司**

**LQS350 Cutting Machine**

|  |  |
| --- | --- |
| 产品代码Product Code | **LQS350** |
| 发动机型号Engine Model | EX270/177F |
| 发动机类型Engine Type | Four-stroke, single cylinder, forced air-cooling |
| 排量Displacement (cc) | 270 |
| 最大功率Max. Output (kw/r/min) | 6.0/3600 |
| 油耗Fuel Consumption (g/kw.h) | 313 |
| 刀片直径Blade Diameter (mm) | 350 |
| 切割深度Cut Depth (mm) | 120 |
| 最大切割深度Max. Cut Depth Adjust | Screw Rod Type |
| 推进方式Propel Type | Hand Type |
| 怠速Idle Revolution | 1400±150 |
| 工作转速Work Revolution (r.min) | 3600 |
| 水箱容量Water Tank (L) | 26 |
| 产品尺寸Product size (mm) | 1000\*810\*560 |
| 包装尺寸Packing size (mm) | 800\*460\*1100 |
| 净重Net Weight (kg) | 140 |
| 毛重Gross Weight (kg) | 165 |

**Product characteristics:**

1. These floor saws offer a cutting performance second to none in this class of machines.

2、The torque transmitted to the diamond blade and the center of gravity located over the cutting shaft have beenmatched so efficiently.

3、That the majority of the engine’s power output goesthere where it is needed,into the asphalt or the conctete.

4、These two features result in cuts up to 20 percent faster than comparable products